{"text_format":"1","workbook":"xlsx","n_sheets":4,"sheets":["Sensitivity","SpectraPLUS Instructions","SignalScope Pro Instructions","Revision History"],"not_rendered":{"charts":0,"images":8,"macros":1,"external_links":0,"defined_names":1,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900"}

{"sheet":"Sensitivity","index":0,"n_rows":30,"n_cols":24,"rows_kept":30,"cut":false,"hidden":false,"merged":[[2,0,3,0],[2,2,3,2],[2,3,3,3],[2,4,3,4],[2,5,3,5],[2,1,3,1],[0,2,0,5],[2,12,2,13],[2,14,2,15],[2,16,2,17],[2,18,2,19],[1,12,1,23],[2,20,2,21],[2,22,2,23],[2,10,2,11],[2,6,3,6],[2,7,2,8],[2,9,3,9]]}
[null,null,"Press 'Scan' to read calibration information from all \nattached Digiducer sensors. \nRequires Macro's to be enabled."]
[null,null,"TEC 29-Dec-2015",null,null,null,null,null,null,null,null,null,"Scale Factors to convert the specifed input format to engineering units "]
["Sensor","Model","Serial #","Calibration\nDate\nDD-MMM-YYYY","Channel A\nCounts / (m/s2)","Channel B\nCounts / (m/s2)","Comment","SpectraPLUS-RT and SpectraPLUS-SC\nCalibration Tab, Reference 1 g RMS",null,"24 Bit Sample (g RMS)\n(VibeRMS, VibePro)","g/Full Scale\n(SignalScope Pro)",null,"24 Bit Integer Sample (g)\n(WaveIn)",null,"24 Bit Integer Sample (m/s2)\n(WaveIn)",null,"Scaled Value, -1 to 1, (g)\n(Matlab, M+P SmartOffice)",null,"Scaled Value, -1 to 1, (m/s2)\n(Matlab, M+P SmartOffice)",null,"% Full Scale, (g)\n(-100% to 100%)",null,"% Full Scale, (m/s2)\n(-100% to 100%)"]
[null,null,null,null,null,null,null,"Left","Right",null,"Chan A (CH1)","Chan B (CH2)","Chan A (CH1)","Chan B (CH2)","Chan A (CH1)","Chan B (CH2)","Chan A (CH1)","Chan B (CH2)","Chan A (CH1)","Chan B (CH2)","Chan A (CH1)","Chan B (CH2)","Chan A (CH1)","Chan B (CH2)"]
[null,null,null,null,null,null,null,{"$f":"IF(ISBLANK($A5),\"\",E5*(9.80665/SQRT(2))/(2^24)*4*100)","v":""},{"$f":"IF(ISBLANK($A5),\"\",F5*(9.80665/SQRT(2))/(2^24)*4*100)","v":""},{"$f":"IF(ISBLANK($A5),\"\",1/(9.80665*$E5*SQRT(2)))","v":""},{"$f":"IF(ISBLANK($A5),\"\",POWER(2,23)/(9.80665*$E5))","v":""},{"$f":"IF(ISBLANK($A5),\"\",POWER(2,23)/(9.80665*$F5))","v":""},{"$f":"IF(ISBLANK($A5),\"\",1/(9.80665*$E5))","v":""},{"$f":"IF(ISBLANK($A5),\"\",1/(9.80665*$F5))","v":""},{"$f":"IF(ISBLANK($A5),\"\",1/($E5))","v":""},{"$f":"IF(ISBLANK($A5),\"\",1/($F5))","v":""},{"$f":"IF(ISBLANK($A5),\"\",(2^23)/(9.80665*$E5))","v":""},{"$f":"IF(ISBLANK($A5),\"\",(2^23)/(9.80665*$F5))","v":""},{"$f":"IF(ISBLANK($A5),\"\",(2^23)/($E5))","v":""},{"$f":"IF(ISBLANK($A5),\"\",(2^23)/($F5))","v":""},{"$f":"IF(ISBLANK($A5),\"\",(2^23)/(100*9.80665*$E5))","v":""},{"$f":"IF(ISBLANK($A5),\"\",(2^23)/(100*9.80665*$F5))","v":""},{"$f":"IF(ISBLANK($A5),\"\",(2^23)/(100*$E5))","v":""},{"$f":"IF(ISBLANK($A5),\"\",(2^23)/(100*$F5))","v":""}]
[null,null,null,null,null,null,null,{"$f":"IF(ISBLANK($A6),\"\",E6*(9.80665/SQRT(2))/(2^24)*4*100)","v":""},{"$f":"IF(ISBLANK($A6),\"\",F6*(9.80665/SQRT(2))/(2^24)*4*100)","v":""},"","","","","","","","","","","","","","",""]
[null,null,null,null,null,null,null,"","","","","","","","","","","","","","","","",""]
[null,null,null,null,null,null,null,"","","","","","","","","","","","","","","","",""]
[null,null,null,null,null,null,null,"","","","","","","","","","","","","","","","",""]
[null,null,null,null,null,null,null,"","","","","","","","","","","","","","","","",""]
[null,null,null,null,null,null,null,"","","","","","","","","","","","","","","","",""]
[null,null,null,null,null,null,null,"","","","","","","","","","","","","","","","",""]
[null,null,null,null,null,null,null,"","","","","","","","","","","","","","","","",""]
[null,null,null,null,null,null,null,"","","","","","","","","","","","","","","","",""]
[null,null,null,null,null,null,null,"","","","","","","","","","","","","","","","",""]
[null,null,null,null,null,null,null,"","","","","","","","","","","","","","","","",""]
[null,null,null,null,null,null,null,"","","","","","","","","","","","","","","","",""]
[null,null,null,null,null,null,null,"","","","","","","","","","","","","","","","",""]
[null,null,null,null,null,null,null,"","","","","","","","","","","","","","","","",""]
[null,null,null,null,null,null,null,"","","","","","","","","","","","","","","","",""]
[null,null,null,null,null,null,null,"","","","","","","","","","","","","","","","",""]
[null,null,null,null,null,null,null,"","","","","","","","","","","","","","","","",""]
[null,null,null,null,null,null,null,"","","","","","","","","","","","","","","","",""]
[null,null,null,null,null,null,null,"","","","","","","","","","","","","","","","",""]
[null,null,null,null,null,null,null,"","","","","","","","","","","","","","","","",""]
[null,null,null,null,null,null,null,"","","","","","","","","","","","","","","","",""]
[null,null,null,null,null,null,null,"","","","","","","","","","","","","","","","",""]
[null,null,null,null,null,null,null,"","","","","","","","","","","","","","","","",""]
[null,null,null,null,null,null,null,"","","","","","","","","","","","","","","","",""]
[null,null,null,null,null,null,null,"","",null,"","","","","","","","","","","","","",""]

{"sheet":"SpectraPLUS Instructions","index":1,"n_rows":62,"n_cols":1,"rows_kept":62,"cut":false,"hidden":false,"merged":[]}
["This should normally not be necessary but we have gotten reports of issues reading the calibration "]
["on computers with Asian versions of Windows."]
[]
["1. Press 'I/O' button on main tool bar"]
[]
[]
[]
[]
[]
[]
["2. Select 333D01 device from 'Input Device' pull down menu."]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
["3. Select the calibration tab"]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
["4. Normally, you can just press 'Read calibration data from device'.  This will display the sensor serial number and calibration date and set the left and right sensitivity."]
[]
["If that doesn't work, the sensitivity scaling data can be entered manually"]
["5. Confirm 'Reference Signal Parameters' are Level 1.0000, RMS, and Units are Acceleration (G)"]
["6. Enter Left and Right 'Measured Levels' from the 'Sensitivity' page of this spreadsheet."]

{"sheet":"SignalScope Pro Instructions","index":2,"n_rows":135,"n_cols":1,"rows_kept":135,"cut":false,"hidden":false,"merged":[]}
["SignalScope Pro Instructions"]
["A Faber Acoustical Application"]
["Note: The base SignalScope does not support g's as basic type"]
[]
["SignalScope Pro version 4.0 or later automatically reads and uses the programmed sensitivity.  This procedure is not necessary."]
[]
["The upgraded Data Acquistion upgrade to SignalScope version 5.0 or later does not need this procedure."]
[]
["1. Plug in 333D01 using camera adapter. Start SignalScope Pro and press the gears icon in upper right."]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
["2. Press 'I/O Device Configuration'"]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
["3.  Select Device Units of 'FS'.  \nNote: you can set the sample rate here as well.  \nPress 'Input Channels'"]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
["4. In 'ALL CHANNELS', select units of g\npress CH1 Calibrate "]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
["5. Type in number from Sensitivity page for CH1 (Ch A) into Input Sensitivity"]
["Note: dB scale is relative 1 g RMS which is defined in the reference field"]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
["6. Go back to previous screen and select Ch2.  Repeat process."]

{"sheet":"Revision History","index":3,"n_rows":6,"n_cols":4,"rows_kept":6,"cut":false,"hidden":false,"merged":[]}
["Version","Date","Who","Change"]
["1.00","2014-10-07","RN","Initial Release"]
["1.01","2014-10-09","TEC","Column J did not include G in the conversion.\nUpdated SignalScope Pro section to say this is not necessary if you have a current release"]
[1.02,"2015-02-02","TEC","Add new scale factor for VibeRMS and VibePro"]
[1.03,"2015-06-05","TEC","Added calculations for scale factors for Pioneer Hill Software SpectraPLUS-RT and SpectraPLUS-SC"]
[1.04,"2015-12-29","TEC","Added support for 333D02, and MB63 - Renamed to Digiducer Calibration Decoder"]